**List of Tables**

|  |  |
| --- | --- |
|  |  |
| Table 1 Terrain with non-rectangular obstacle applied with HPA\* pathfinding algorithm | 6 |
| Table 2 Performance of HPA\* on static obstacles | 8 |
| Table 3 Performance of HPA\* on dynamic obstacles | 8 |
| Table 4 10% blocked node in grid map | 20 |
| Table 5 50% blocked node in grid map | 21 |
| Table 6 Terrain with non-rectangular obstacle applied with navmesh on HPA\* pathfinding algorithm | 25 |
| Table 7 Unit traverse different transitions | 28 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**List of Figures**

|  |  |
| --- | --- |
|  |  |
| Figure 1. Terrain with non-rectangular obstacle | 5 |
| Figure 2. HPA\* applied on terrain from figure 1.1.1 | 6 |
| Figure 3. Interaction of the unit to dynamic obstacle (different unit) on HPA\* | 7 |
| Figure 4. Different placement of transitions on the same entrance | 9 |
| Figure 5. Interaction of HPA\* algorithm to non-rectangular obstacles. | 25 |
| Figure 6. Interaction of proposed algorithm to non-rectangular obstacle | 25 |
| Figure 7. Unit interaction to dynamic obstacles on HPA\* | 27 |
| Figure 8. Unit interaction to dynamic obstacle on proposed algorithm | 27 |
| Figure 9 Unit circles around the non-rectangular obstacle | 33 |
| Figure 10 Unit passes through the area between the non-rectangular obstacle | 33 |
| Figure 11 Unit stops when encountering dynamic obstacle | 34 |
| Figure 12 Unit passes towards a dynamic obstacle | 34 |
|  |  |
|  |  |